\*\*\* Some of the prep work will begin prior to the close of business, any reloads would be scheduled later in the evening (5:00pm and later) \*\*\*

\*\*\* Open a cmd session and run a continuous ping to the switch \*\*\*

SWITCHES & MODELS (see below)

US-ADS-OCAL-MDF-SW01 10.129.43.1 WS-C3850-48P

show version:

(note: System image file is "flash:cat3k\_caa-universalk9.SPA.03.06.05.E.152-2.E5.bin")

\*\* Switch is in bundle mode \*\*

show boot

---------------------------

Switch 2

---------------------------

Current Boot Variables:

BOOT variable = flash:cat3k\_caa-universalk9.SPA.03.06.05.E.152-2.E5.bin;

Boot Variables on next reload:

BOOT variable = flash:cat3k\_caa-universalk9.SPA.03.06.05.E.152-2.E5.bin;

Allow Dev Key = yes

Manual Boot = no

Enable Break = no

\*\*\*\*\*\*\*\*\*\*\*

Convert to install mode:

dir flash:

rename: packages.conf - to- old.packages.conf

dir flash-1:

del: packages.conf

dir flash-3:

del: packages.conf

software expand running to flash

dir flash: (verify packages.conf exists)

dir flash-1: (verify packages.conf exists)

dir flash-3: (verify packages.conf exists)

Config t

boot system switch all flash: packages.conf

ctrl-z

wr

show boot - (you should see the new boot referencing the packages.conf)

reload